**PLEASE PARK VEHICLES IN YOUR DRIVEWAY AND/OR BEYOND THE LIMITS OF THE STREET SCHEDULED FOR APPLICATION. SEE SCHEDULE**

**MICROSURFACING: The Application**

* Micro-surfacing is a mixture of asphalt emulsion and aggregate

(crushed stone, gravel, and sand) applied to the road. The

emulsion is modified with polymers and other ingredients so it

cures more quickly.

* The benefits include a very smooth and esthetically pleasing

surface with increased durability by sealing the existing

pavement, improved ride experience, improved road safety

by increasing surface friction, bolsters unstable life of existing

pavement, environmentally friendly.

* Residents can expect 4-6 hours of delay to allow for the

application to cure completely. Proper cure time is estimated to

be 4-6 hours once the application has been applied.

**IN CASE OF: Inclement Weather and/or Mechanical Issues**

* Weather, mechanical problems or other delays may prevent completion of street(s) on the scheduled day. If this happens, work will resume the next working day. Microsurfacing can also be postponed by the threat of rain. Work will resume on the first day the asphalt surface conditions are met and favorable weather forecasts without any additional notice.

**STREET / ROADWAY ACCESSIBILITY: Driveways and Off-Site Parking Areas**

* A few streets will be "CLOSED", during the application. Most streets will have Limited “Ingress/Egress" during Microsurfacing Operations. Curing of the Application will dictate the timing, and the amount of access residents will have to driveways.
* Emergency Services will have "TOTAL" access to all streets including during the application process.